# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: All-terrain vehicle p 1 /11**

**Publication reference: РД-02-29-82/16.05.2019/PUC Tender 02**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offered specifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | 4x4  Max power: 110kW/150ks  Maximum torque: 400/1600-2000 Nm/o/min  Maximum speed: 170 km/h  Acceleration 0-100km/h:13,23 km/h  ABS (Antilock Brake System)  BA (Brake assistance)  EBD (Electronic Brake force Distribution)  TRC (Electronic Traction Control)  VSC (Vehicle Stability Control)  17-inch steel wheels  Tires dimension 225170 R17 (TSC)  Tires dimension 265165 R17 (for EC and DC)  Daylight  Spare tire |  |  |  |