# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of equipment for the Promoting center in Botevgrad p 1/2**

**Publication reference:** CB007.2.11.224 – LP - Supply 1

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | -  Outdoor video audio system with vertical LED video screen - 1pc, size B = 500cm (+/-5%), H = 290cm (+/-5%), with 6mm  (+/-5%) inter pixel distance, hanging on a metal supporting structure of an installation wall, Brightness (cd / ㎡ ) ≥5500nit, LED type SMD 3535 or equivalent, Operating Temperature (℃) min. -20 ~ 50, Pixels dot/㎡ min. 15625, LED Life (hrs) Min 50,000 Processor LVP or equivalent - 1 piece, Hardware Controller Server and Screen Configuration Software for multimedia broadcasting, interactive system, connectors, cables, ancillary tools for installation |  |  |  |
| **2** | - Telepresence mode - Multipoint, Telepresence mode - two 50" (+/- 10%) LCD or equivalent screen, compiled by “End Point”, “Infrastructure” and devices type Multipoint Central Unit- MCU or equivalent |  |  |  |
| **3** | - Multimedia system for indoor conditions with vertical LED video screens - 2pcs, sizes B = 150cm (+/- 5%), H = 300cm (+/- 5%), with 2.5 pixels spacing (+/- 5%), floor standing, min 50,000 hrs, LVP or equivalent - 2 ps processors, hardware and software for configuration of screens, connectors, cables, ancillary tools for installation. |  |  |  |
| **4** | - Digital Information Displays 43" (+/- 10%) multi touch - 3pcs, organized in network with centralized management /integrated computer for management, integrated network module / |  |  |  |