# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of Set of special fire protection clothes p 1 /…**

**Publication reference:** **CB007.2.31.131-PP2-02**

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1.** | **Set of special fire protection clothes** |  |  |  |
|  | Fire protection costume – 15 pcs.:   * Composed of 2 (two) parts – upper and lower;   The fire protection costumes must meet the following requirements:   * Fire resistant; * Breathable matter; * Waterproof outer sheath; * Reflective strip resistant to flames on the chest, back, arms and legs for optimum visibility during day and night; * Protection level – xf2, xr2, y1, z2; * Approval – EN 469:2005 + A1:2006; EN 340:2003.   Fire protection boots – 15 pcs.:   * To ensure access to hard-to-reach areas; * To prevent volunteers from injuries; * Material – upper part of heat-insulating and chemically resistant fireproof rubber; rubber sole; refractory, resistant to liquid fuel and slipping; * Cold-insulating outer construction; * An average piece of steel, resistant to sharp objects; * Cotton linen lining; * Steel finger protector (EN ISO 20345); * Application – for open fire operation; * Personal protective equipment – Category III; * Approval: EN 659: 2003 + A1: 2008; Directive 96/ 98/ EU.   Fire protection gloves – 15 pcs.:   * To protect volunteers hands from injuries and burns; * Material – natural calf leather; * Narrowing of the wrist by trapping and closing type; * Sheathing with insulating material, resistant to incision (100 para-aramid; * Application – for open fire operation; * Personal protective equipment – Category III; * Approval: EN 659: 2003 + A1 : 2008; Directive 96/ 98/ EU. |  |  |  |